**OpenWLS(WellLoggingSystem)**

There’re four projects

* Client: WPF GUI
* Server: Web API server
* Edge: none-eth port surface panel manger, playback;
* PLT1: an exemplary tool library

Server

Client

Edge

Surface Equipment

Downhole toolstring

TCP/IP

HTTP

TCP/IP

USB…